Chapter 3

User exit subroutines

This section describes the user exit subroutine.

39

40 EMSOL Subroutine Library: Version 0

ems itru

This subroutine is called after every Iiterufreq iterations, or after resetting the current model.

Specification

call ems itru(dspace, dspace, reason, userrtcd)

On entry

dspace

is the user-provided work area.

Specified as: a one-dimensional real array of doublewords.

dspace

is the integer version of the work area.

Specified as: a one-dimensional integer array of fullwords.

reason

is the situation where ems itru is called.

If reason = 1, the subroutine is called after a primal iteration of

ems sslv.

If reason = 3, the subroutine is called after a resetting the current model during ems sslv.

Specified as: a fullword integer.

usrrtcd

is the user return code from the user exit subroutine. Specified as: a fullword integer.

On return

dspace

is the user-provided work area.

Returned as: a one-dimensional real array of doublewords.

dspace

is the integer version of the work area.

Returned as: a one-dimensional integer array of fullwords.

usrrtcd

is the user return code from the user exit subroutine, where:

If usrrtcd = 3, EMSOL acts as if the maximum number of iterations has been reached.

If usrrtcd = 99, then the current model is reset.

Chapter 3 User exit subroutines 41 Returned as: a fullword integer.

Notes